Ontario Low Water Response Program - Calculated Indexes, 2026
January 
[bookmark: _Hlk36040003]
Precipitation – 1 month
	Station
	Average January, mm
	Actual January 2026
	
Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	60.9
	49.8
	82%
	Normal

	Port Perry
	64.9
	13.8
	21%
	Level 3

	Average for Watershed
	62.9
	31.8
	51%
	Level 2


Flow
	Station
	Minimum monthly summer flow, m3/sec
	January 2026 
mean, 
m3/sec
	January 2026,  
 % of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	8.8
	109%
	Normal

	Mariposa Brook at Little Britain
	0.194
	3.827
	1973%
	Normal

	Blackstock Creek near Blackstock 
	0.041
	0.267
	650%
	Normal

	Pigeon River at Lotus
	0.253
	0.235
	93%
	Normal


February 
Precipitation
[bookmark: _Hlk36040022]Precipitation – 1 month
	Station
	Average February, mm
	Actual February 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	56.9
	32.6
	57%
	Level 2

	Port Perry
	45.9
	31.6
	69%
	Level 1

	Average for watershed
	51.4
	32.1
	62%
	Level 1



Flow
	Station
	Minimum monthly summer flow, m3/sec
	February 2026 - 
mean, 
m3/sec
	February 2026,  
 % of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	7.323
	90%
	Normal

	Mariposa Brook at Little Britain
	0.194
	1.699
	876%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.149
	364%
	Normal

	Pigeon River at Lotus
	0.253
	0.235
	93%
	Normal




MARCH 
Precipitation
[bookmark: _Hlk36040190]Precipitation – 1 month
	Station
	Average March, mm
	Actual March 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	52.7
	96.5
	183%
	Normal

	Port Perry
	53.1
	94.4
	178%
	Normal

	Average for watershed
	52.9
	95.5
	180%
	Normal


Precipitation – 3 months
	Station
	Average 3-month, January-March,
mm
	Actual 3-month
January – March 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	170.6
	178.9
	105%
	Normal

	Port Perry
	163.9
	139.8
	85%
	Normal

	Average for watershed
	167.3
	159.4
	95%
	Normal


Flow
	Station
	Minimum monthly summer flow, m3/sec
	March 2026 - 
mean, 
m3/sec
	March 2026,  
 % of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	43.131
	532%
	Normal

	Mariposa Brook at Little Britain
	0.194
	10.51
	5419%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.825
	2012%
	Normal

	Pigeon River at Lotus
	0.253
	0.473
	187%
	Normal









April
Precipitation
Precipitation – 1 month
	Station
	Average April, mm
	Actual April 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Emily PP
	65.2
	116.2
	178%
	Normal

	Ken Reid CA
	85.7
	151.9
	177%
	Normal

	Mariposa Brook GS
	65.0
	121.4
	187%
	Normal

	Port Perry
	67.9
	119
	156%
	Normal

	Average 
	71
	127.1
	179%
	Normal



Precipitation – 3 months
	Station
	Average 3-month, February-April,
mm
	Actual 3-month
February – April 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	188.6
	281
	149%
	Normal

	Port Perry
	166.9
	245.0
	147%
	Normal

	Average 
	177.8
	263
	148%
	Normal



Flow
	Flow Station
	Minimum monthly summer flow, m3/sec
	April 2026 -
mean,
m3/sec
	April 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	87.09
	1075%
	Normal

	Mariposa Brook at Little Britain
	0.194
	9.976
	5142%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.919
	2240%
	Normal

	Pigeon River at Lotus
	0.253
	0.675
	267%
	Normal



May 

Precipitation – 1 month


	Station
	Average May, mm
	Actual May 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Trent Lakes Municipal Office 
	97.8
	80.9
	83%
	Normal

	Emily PP
	83.8
	90.2
	108%
	Normal

	Ken Reid CA
	76.3
	79.3
	104%
	Normal

	Mariposa Br. GS
	83.8
	85.9
	103%
	Normal

	Port Perry
	82.1 
	70.9
	86%
	Normal

	Blackstock GS
	106.9
	125.4
	117%
	Normal

	Average
	89.4
	76.1
	85%
	Normal



[bookmark: _Hlk201045655]
Precipitation – 3 months

	Station
	Average 3-month, March-May,
mm
	Actual 3-month
March-May 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	204.4
	327.7
	160
	Normal

	Port Perry
	203.1
	284.3
	140%
	Normal

	Average
	203.8
	306
	150%
	Normal



Flow

	Station
	Minimum monthly summer flow, m3/sec
	May 2026 -
mean,
m3/sec
	May 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	21.798
	269%
	Normal

	Mariposa Brook at Little Britain
	0.194
	2.986
	1539%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.211
	514%
	Normal

	Pigeon River at Lotus
	0.253
	0.320
	126%
	Normal


[bookmark: _Hlk201045694]
June

[bookmark: _Hlk50542056]Precipitation – 1 month
	Station
	Average June, mm
	Actual June 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Trent Lakes Municipal Center
	90.6
	108.8
	120%
	Normal

	Emily PP
	82.6
	70.6
	85%
	Normal

	Ken Reid CA
	92.8
	71.9
	77%
	Level 1

	Mariposa Br. GS
	79.2
	84.7
	107%
	Normal

	Port Perry
	106.6 
	113.1
	106%
	Normal

	Blackstock Cr. GS
	96.8
	123
	127%
	Normal

	Pigeon River GS
	96.8
	69.4
	72
	Level 1

	Average
	92
	91.6
	99%
	Normal




[bookmark: _Hlk201045452]Precipitation – 3 months
	Station
	Average 3-month, 
April-June,
mm
	Actual 3-month
April-June 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	233.1
	303.1
	130%
	Normal

	Mariposa Br. GS
	220.0
	292
	133%
	Normal

	Port Perry
	256.6
	303
	118%
	Normal

	Average 
	236.6
	299.4
	127%
	Normal










Flow

	Station
	Minimum monthly summer flow, m3/sec
	June 2026 -
mean, m3/sec
	June 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	22.494
	278%
	Normal

	Mariposa Brook at Little Britain
	0.194
	3.690
	1902%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.126
	304%
	Normal

	Pigeon River at Lotus
	0.253
	0.238
	94%
	Normal





[bookmark: _Hlk204239174]July
Precipitation – 1 month
	Station
	Average July, mm
	Actual July, 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Trent Lakes Municipal Center
	82.2
	83
	101%
	Normal

	Emily PP
	75.8
	78.6
	104%
	Normal

	Ken Reid CA
	76.8
	77.7
	101%
	Normal

	Mariposa Br. GS
	72.4
	73.8
	102%
	Normal

	Port Perry
	74.9
	114.1
	152%
	Normal

	Pigeon R. GS
	105.4
	90.8
	86%
	Normal

	Average for Watershed
	81.3
	86.3
	106%
	Normal



Precipitation – 3 months	

	[bookmark: _Hlk110501193][bookmark: _Hlk50542774]Station
	Average 3-month, May-July, 
mm
	Actual 3-month,
May-July 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Trent Lakes Municipal Center
	270.6
	272.7
	101%
	Normal

	Emily PP
	237.3
	239.4
	101%
	Normal

	Ken Reid CA
	237.3
	228.9
	96%
	Normal

	Mariposa Br. GS
	228.9
	             244.4
	107%
	Normal

	Port Perry
	275.1
	298.1
	108%
	Normal

	Pigeon Rv. GS
	308.4
	225.6
	73%
	Normal

	Average for Watershed
	267
	251.5
	97%
	Normal


[bookmark: _Hlk204239662]



Flow 

	Station
	Minimum monthly summer flow, m3/sec
	July 2026 -
mean,
m3/sec
	July 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	8.116
	100%
	Normal

	Mariposa Brook at Little Britain
	0.1940
	2.219
	1144%
	Normal

	Blackstock Creek near Blackstock
	0.041
	0.079
	193%
	Normal

	Pigeon River near Lotus
	0.228
	0.226
	99%
	Normal


   

August

Precipitation – 1 month
	Station
	Average August, mm
	Actual August, 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Trent Lakes Municipal Center
	78.0
	
	
	

	Emily PP
	85.7
	
	
	

	Ken Reid CA
	76.8
	
	
	

	Mariposa Br. GS
	86.4
	
	
	

	Blackstock Cr. GS
	87.10
	
	
	

	Port Perry
	87.10
	
	
	

	Pigeon Rv. GS
	87.10
	
	
	

	Average for Watershed
	80.5
	
	
	



Precipitation – 3 months

	Station
	Average 3-month, June-August,
mm
	Actual 3-month,
June-August 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	250.8
	
	
	

	Trent Lakes Municipal Office
	250.8
	
	
	

	Emily PP
	240.5
	
	
	

	Ken Reid CA
	240.5
	
	
	

	Mariposa Br. GS
	214.2
	
	
	

	Blackstock Cr. GS
	288.5
	
	
	

	Port Perry
	266.9
	
	
	

	Average for Watershed
	252.4
	
	
	



Flow - August

	Station
	Minimum monthly summer flow, m3/sec
	August 2026 -
mean,
m3/sec
	August,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	
	
	

	Mariposa Brook at Little Britain
	0.194
	
	
	

	Blackstock Creek near Blackstock
	0.041
	
	
	

	Pigeon River near Lotus
	0.260
	
	
	





September
[bookmark: _Hlk52455065]Precipitation – 1 Month
	Station
	Average September, mm
	Actual September 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	89.8
	
	
	

	Trent Lakes Municipal Center
	100.2
	
	
	

	Emily PP
	88.2
	
	
	

	Ken Reid CA
	77.4
	
	
	

	Mariposa Br. GS
	88.6
	
	
	

	Blackstock Cr. GS
	91.2
	
	
	

	Port Perry
	87.3
	
	
	

	Pigeon Rv. GS
	91.2
	
	
	

	Average for Watershed
	89.0
	
	
	



[bookmark: _Hlk55998899]Precipitation – 3 Months
	Station
	Average 3-month, 
July-September, mm
	Actual 3-month
July-September 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	260.4
	
	
	

	Municipality of Trent Lakes Office
	260.4
	
	
	

	Emily PP
	NA
	
	
	

	Ken Reid CA
	202.8
	
	
	

	Mariposa Br. GS
	250.5
	
	
	

	Blackstock Cr. GS
	283.0
	
	
	

	Port Perry
	247.6
	
	
	

	Pigeon Rv. GS
	283.0
	
	
	

	Average for Watershed
	254.4
	
	
	


Flow

	Station
	Minimum monthly summer flow, m3/sec
	September 2026 -
mean,
m3/sec
	September 2026,
% of minimum monthly summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	
	
	

	Mariposa Brook at Little Britain
	0.194
	
	
	

	Blackstock Creek near Blackstock
	0.041
	
	
	

	Pigeon River near Lotus
	0.254
	
	
	





[bookmark: _Hlk147825170]October
Precipitation – 1 Month
	Station
	Average October, mm
	Actual October 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	97.2
	
	
	

	Trent Lakes Office
	72.5
	
	
	

	Emily PP
	73.3
	
	
	

	Ken Reid CA
	72.5
	
	
	

	Mariposa GS
	73.3
	
	
	

	Blackstock
	77.9
	
	
	

	Port Perry
	74.9
	
	
	

	Pigeon Rv. GS
	77.9
	
	
	

	Average for Watershed
	74.7
	
	
	



Precipitation – 3 Months
	Station
	Average 3-month, August-October, mm
	Precipitation August – October
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	245.3
	
	
	

	Mariposa GS
	249.9
	
	
	

	Pigeon Rv. GS
	249.9
	
	
	

	Blackstock GS
	256.2
	
	
	

	Port Perry
	236.1
	
	
	

	Emily PP
	245.3
	
	
	

	Trent Lake Municipal Office
	245.3
	
	
	

	Average for Watershed
	245.5
	
	
	






[bookmark: _Hlk147825420]Flow
	Station
	Minimum monthly summer flow, m3/sec
	October 2026 -
mean,
m3/sec
	October 2026,
% of minimum monthly summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	
	
	

	Mariposa Brook at Little Britain
	0.194
	
	
	

	Nonquon River near Port Perry
	0.032
	
	
	

	Blackstock Creek near Blackstock
	0.041
	
	
	

	Pigeon River near Lotus
	0.254
	
	
	





November
Precipitation – 1 Month
	Station
	Average November, mm
	Actual November 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	109.3
	
	
	

	Ken Reid CA
	67.8
	
	
	

	Port Perry
	83.2
	
	
	

	Average for Watershed
	86.7
	
	
	



Precipitation – 3 Months
	Station
	Average 3-month, September-November, mm
	Actual 3-month
   September-November 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Indian Point PP
	306.7
	
	
	

	Ken Reid CA
	226.5
	
	
	

	Port Perry
	245.4
	
	
	

	Average for Watershed
	256.0
	
	
	



Flow
	Station
	Minimum monthly summer flow, m3/sec
	November 2026 –
mean, m3/sec
	November 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	
	
	

	Mariposa Brook at Little Britain
	0.194
	
	
	

	Blackstock Creek near Blackstock
	0.041
	
	
	

	Pigeon River near Lotus
	0.247
	
	
	



December
Precipitation – 1 Month
	Station
	Average December, mm
	Actual December 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	76.0
	
	
	

	Port Perry
	60.0
	
	
	

	Average for Watershed
	68
	
	
	



Precipitation – 3 Months
	Station
	Average 3-month, October-December, mm
	Actual 3-month
   October-December 2026
	Ontario Low Water Response Conditions Level

	
	
	mm
	%
	

	Ken Reid CA
	228.3
	
	
	

	Port Perry
	218.1
	
	
	

	Average for Watershed
	223.2
	
	
	



Flow
	Station
	Minimum monthly summer flow, m3/sec
	December 2026 –
mean, m3/sec
	December 2026,
% of minimum summer flow
	Ontario Low Water Response Conditions Level

	Burnt River near Burnt River
	8.10
	
	
	

	Mariposa Brook at Little Britain
	0.194
	
	
	

	Blackstock Creek near Blackstock
	0.041
	
	
	

	Pigeon River near Lotus
	0.247
	
	
	















